{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Feuil1","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Équipements","Durée de vie","Franchise","Abattement par année après franchise","Valeur résiduelle à la charge du locataire après durée de vie si dégradations"]
["Appareils sanitaires","20 ans","5 ans",0.05,0.25]
["Ballon d’eau chaude","10 ans","2 ans",0.1,0.2]
["Carrelage/faïence murale","20 ans","5 ans",0.05,0.25]
["Carrelage, parquet","20 ans","5 ans",0.05,0.25]
["Climatiseurs","5 ans","1 an",0.2,0.2]
["Electricité (tableau, réseau)","20 ans","5 ans",0.05,0.25]
["Menuiseries intérieures et extérieures","20 ans","5 ans",0.05,0.25]
["Meuble sous évier","10 ans","2 ans",0.1,0.2]
["Moquette","7 ans","1 an",0.15,0.1]
["Peinture, papier","7 ans","1 an",0.15,0.1]
["Persiennes en bois ou plastique","10 ans","2 ans",0.1,0.2]
["Plomberie","15 ans","5 ans",0.08,0.2]
["Revêtement plastique sol","10 ans","2 ans",0.1,0.2]
["Robinetterie","10 ans","2 ans",0.1,0.2]
["Serrurerie, quincaillerie","10 ans","2 ans",0.1,0.2]
["Stores","5 ans","1 an",0.2,0.2]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}